(footprint "NEMA17" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Unnamed StepUp generated footprint")
  (attr through_hole)
  (fp_text reference "FC_" (at 0 1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 039df245-82c0-4810-aa25-b5a44f38de10)
  )
  (fp_text value "Val_" (at 0 -1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3e183324-fc47-483a-a447-e796e372522a)
  )
  (fp_text user "EDIT PAD NUMBERS" (at 0 -2) (layer "Cmts.User")
      (effects (font (size 1 1) (thickness 0.2) italic))
    (tstamp 2615b9c7-84bb-4e43-aa91-cb8e2de887d3)
  )
  (fp_text user "${REFERENCE}" (at 0 1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 33e36b7b-63dd-4b4f-981a-7c75f58fb3b7)
  )
  (fp_line (start -21 15.5) (end -21 -15.5)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp 5d174f66-abee-4790-b25c-e3f72794ee95))
  (fp_line (start -15.5 -21) (end 15.5 -21)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp b50591ae-003d-4b3c-b235-07cee390ee11))
  (fp_line (start 15.5 21) (end -15.5 21)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp 882d89fb-969b-4d55-96a5-8edb988adc95))
  (fp_line (start 21 -15.5) (end 21 15.5)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp 8d3ad6f3-b483-4004-a61c-3d8c90b0d677))
  (fp_arc (start -21 -15.5) (mid -19.389087 -19.389087) (end -15.5 -21)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp 1a3f996f-2b91-499c-aa68-cb1ee2323ab2))
  (fp_arc (start -15.5 21) (mid -19.389087 19.389087) (end -21 15.5)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp 973c8c8a-1560-4def-91f5-9edb715c9f08))
  (fp_arc (start 15.5 -21) (mid 19.389087 -19.389087) (end 21 -15.5)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp dc708ccd-8214-4805-820d-4102bbcbd543))
  (fp_arc (start 21 15.5) (mid 19.389087 19.389087) (end 15.5 21)
    (stroke (width 0.016) (type solid)) (layer "Edge.Cuts") (tstamp 94afbf5b-6ea1-4396-914a-3bab6f36aebd))
  (fp_circle (center 0 0) (end -2.5 0)
    (stroke (width 0.11) (type solid)) (fill none) (layer "F.Fab") (tstamp 00385018-66f9-4f61-8db2-c07cf2043a69))
  (pad "1" thru_hole circle (at -15.5 -15.5) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp aea59957-23a1-481f-9048-88c4ce547bac))
  (pad "1" thru_hole circle (at -15.5 15.5) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp 5d8e2e1c-919e-49bc-b3c6-54d16d8ce3c4))
  (pad "1" thru_hole circle (at 15.5 -15.5) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp 3d5d0970-a682-4014-80b8-b671ced0e83a))
  (pad "1" thru_hole circle (at 15.5 15.5) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp f6fc9e6d-b0c8-4464-b8a1-0d4d67cccd27))
  (model "/Users/mateijordache/Documents/electronics_projects/lemon-pepper-stepper/mechanical/Unnamed.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
