(footprint "PinHeader_1x05_P1.27mm_SMD" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
  (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.235) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 62ff5690-ff1e-4091-9b1c-85b28086b558)
  )
  (fp_text value "PinHeader_1x05_P1.27mm_SMD" (at 0 4.235) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6c731e36-997f-4c1d-976b-30487e30c065)
  )
  (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1e01c9b9-3d31-4697-95bd-64ca00538654)
  )
  (fp_line (start -4.3 -3.7) (end -4.3 3.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25f38bc9-d653-4646-9659-5aea3daaa1e4))
  (fp_line (start -4.3 3.7) (end 4.3 3.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9128f731-06b9-437f-9ac5-f504b246bed8))
  (fp_line (start 4.3 -3.7) (end -4.3 -3.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d6156db7-05bd-4877-94bc-69d5ee57c73d))
  (fp_line (start 4.3 3.7) (end 4.3 -3.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c450d06-738b-411d-a27b-61d4d7ea6e8a))
  (fp_line (start -1.705 -2.74) (end -1.27 -3.175)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 809c87cf-12dc-496e-97d4-e3a6310dc321))
  (fp_line (start -1.705 3.175) (end -1.705 -2.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 574309e4-35ce-47ef-a773-18681c5b1366))
  (fp_line (start -1.27 -3.175) (end 1.705 -3.175)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 486120b5-f86a-4e61-98e0-9a6725347739))
  (fp_line (start 1.705 -3.175) (end 1.705 3.175)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7dbdc2f6-0f22-49e6-92eb-ab8fa8c713f5))
  (fp_line (start 1.705 -2.74) (end 2.75 -2.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8f977b4-720e-4870-b20a-333c1f0aabda))
  (fp_line (start 1.705 -1.47) (end 2.75 -1.47)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1a00ed6-465a-4021-8ada-6f6458367b5e))
  (fp_line (start 1.705 -0.2) (end 2.75 -0.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7208c986-6317-4f80-935d-d02a11c4e251))
  (fp_line (start 1.705 1.07) (end 2.75 1.07)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79516710-acf2-4b6b-8bdd-13b6f6b002da))
  (fp_line (start 1.705 2.34) (end 2.75 2.34)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60cc5e94-98de-4ef4-a796-fa20b2a6fcbf))
  (fp_line (start 1.705 3.175) (end -1.705 3.175)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 03baa8ed-030c-4a6e-a578-0474df8a6c12))
  (fp_line (start 2.75 -2.74) (end 2.75 -2.34)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 043a3795-0233-497a-bcf7-21e369d47f5c))
  (fp_line (start 2.75 -2.34) (end 1.705 -2.34)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1f292d3e-ef0e-4fc6-bcc5-488514769e44))
  (fp_line (start 2.75 -1.47) (end 2.75 -1.07)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 23bdffca-2864-41c2-999d-d619f208be8a))
  (fp_line (start 2.75 -1.07) (end 1.705 -1.07)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fad50c90-b5b4-43b9-95bf-3cc21b19e08e))
  (fp_line (start 2.75 -0.2) (end 2.75 0.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 33ef79d0-7a4c-4493-8fbc-d0b0d9e4694d))
  (fp_line (start 2.75 0.2) (end 1.705 0.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp acaf232c-27b8-4b93-9e14-de55b0feec9a))
  (fp_line (start 2.75 1.07) (end 2.75 1.47)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79c209c7-1ba3-426d-a75d-4577249545ef))
  (fp_line (start 2.75 1.47) (end 1.705 1.47)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ded5f695-2f57-4a73-addf-bbaae50aaa7e))
  (fp_line (start 2.75 2.34) (end 2.75 2.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e22b9a8-3d22-41fe-aa08-2bd7df2d8283))
  (fp_line (start 2.75 2.74) (end 1.705 2.74)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 36f37999-947a-4b93-8e53-15480bcbe51d))
  (pad "1" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ef08b9df-bfa1-4b49-98bd-6064a41066f6))
  (pad "2" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a4df6b93-f0af-4e63-99a6-15d8d0f30e00))
  (pad "3" smd rect (at 1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a98b79a0-a07a-40b3-aa70-25890f1158e0))
  (pad "4" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2afbf1dd-abd6-4b25-9ec4-c81a43f545da))
  (pad "5" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp de272581-dba8-492d-a4ea-b1bcf368e9a0))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
