(footprint "NEMA14" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Unnamed StepUp generated footprint")
  (attr through_hole)
  (fp_text reference "FC_" (at 0 1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 70f06377-7f08-44d2-bdc4-abaf8f2a5d41)
  )
  (fp_text value "Val_" (at 0 -1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 26a07125-1ac4-4bc6-984c-c1c40c22998a)
  )
  (fp_text user "${REFERENCE}" (at 0 1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2a0e0d82-c2e9-443e-b283-99899dda68d8)
  )
  (fp_line (start -17.5 13) (end -17.5 -13)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp aa6fd337-6cf8-4db4-b1fb-85e518c61dc9))
  (fp_line (start -13 -17.5) (end 13 -17.5)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp 9e0dcf78-a912-4ba1-a605-d89b89c14059))
  (fp_line (start 13 17.5) (end -13 17.5)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp 7ba9296e-a22f-4dbd-ac0b-3b1c33a02ea8))
  (fp_line (start 17.5 -13) (end 17.5 13)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp 9114b86b-ccea-4ff1-9ee2-71f83463de55))
  (fp_arc (start -17.5 -13) (mid -16.181981 -16.181981) (end -13 -17.5)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp f8236d5a-25d4-4d0f-aae4-6268f9eb3c41))
  (fp_arc (start -13 17.5) (mid -16.181981 16.181981) (end -17.5 13)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp 876f9827-c5dd-4812-9689-6034eb29514f))
  (fp_arc (start 13 -17.5) (mid 16.181981 -16.181981) (end 17.5 -13)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp 017431fe-0519-4f39-a328-8260bcde4bb8))
  (fp_arc (start 17.5 13) (mid 16.181981 16.181981) (end 13 17.5)
    (stroke (width 0.15) (type solid)) (layer "Edge.Cuts") (tstamp 380a48a5-14e1-4b6b-9dea-452acc180657))
  (fp_circle (center 0 0) (end -2.5 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 249bb00a-cbc2-4911-bbf0-af2da2a2e0d0))
  (pad "1" thru_hole circle (at -13 -13) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp dca7bc77-b5ae-4cdd-8bd2-2d2a4dc30bfb))
  (pad "1" thru_hole circle (at -13 13) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp 84f65f2d-1e57-4337-9ef0-857a127cb8a6))
  (pad "1" thru_hole circle (at 13 -13) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp 60c60df9-8125-432a-b921-b118e1c20297))
  (pad "1" thru_hole circle (at 13 13) (size 5.8 5.8) (drill 3.1) (layers "*.Cu" "*.Mask") (tstamp 27971454-c6d8-4a02-b4ad-1435accc00b2))
  (model "/Users/mateijordache/Documents/electronics_projects/lemon-pepper-stepper/mechanical/heatsink-nema-14.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
